1. 8-bit input terminals
2. 8-bit output terminals
3. CLK
4. load
5. START: Switch on the processor to execute the instructions
6. RST: clears all register values to zero of processor including instruction and memory register bank, assigns ‘0’ to all counters